1），EasyThreed K7, Can not feeding and retract, nozzle is hot, the filament stuck into gear.

<https://youtu.be/RXp-3S0NjSQ>

2），EasyThreed K7,Can not feeding, nozzle is hot, E motor broken, replace E motor video:

<https://youtu.be/V2ynI0jBMCg>

3），EasyThreed K7, When feeding , light not flash, nozzle not heating up, Nozzle replace video:

<https://youtu.be/kqHHbjmVXBM>

4），EasyThreed K7, X axis not move, X motor replace video

<https://youtu.be/Uz6O_t7StlI>

5），EasyThreed K7, Y motor demaged, Y motor replace video:

<https://youtu.be/DAQUakl5CBM>

6），EasyThreed K7, Z axis not move, Z motor replace video:

<https://youtu.be/gOdYx4DjMwI>

7），EasyThreed K7, X direction print shift , X belt too loose or too tight, X belt adjustment video:

<https://youtu.be/yPpICbNUnyg>

8），EasyThreed K7, Y direction print shift , Y axis belt too loose or too tight, Y belt adjustment video:

<https://youtu.be/F7AaO97Lh0k>

9），EasyThreed K7, Z axis belt too loose or too tight, Z belt adjustment video:

<https://youtu.be/1wNfwZAOmcE>

10），EasyThreed K7, X axis belt come off, re-install video:

<https://youtu.be/29Ns4m8NSeU>

11），EasyThreed K7, Button no function, and online printing not work as well, motherboard dead , motherboard replace video:

<https://youtu.be/Q3nH8pk7t3Q>

12），EasyThreed K7, Feeding has problem, Extruder set replace video:

<https://youtu.be/v0zqibPesfs>